(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "unconnected-(J2-Pad4)")
  (net 5 "Net-(J3-Pad1)")
  (net 6 "Net-(U1-Pad19)")
  (net 7 "Net-(U1-Pad16)")
  (net 8 "Net-(U1-Pad18)")
  (net 9 "Net-(J5-Pad2)")
  (net 10 "Net-(U1-Pad17)")
  (net 11 "unconnected-(U1-Pad1)")
  (net 12 "unconnected-(U1-Pad10)")
  (net 13 "unconnected-(U1-Pad4)")
  (net 14 "unconnected-(U1-Pad5)")
  (net 15 "unconnected-(U1-Pad6)")
  (net 16 "unconnected-(U1-Pad7)")
  (net 17 "unconnected-(U1-Pad8)")
  (net 18 "unconnected-(U1-Pad9)")
  (net 19 "unconnected-(U1-Pad11)")
  (net 20 "unconnected-(U1-Pad12)")
  (net 21 "unconnected-(U1-Pad20)")
  (net 22 "unconnected-(U1-Pad26)")
  (net 23 "unconnected-(U1-Pad21)")
  (net 24 "unconnected-(U1-Pad22)")
  (net 25 "unconnected-(U1-Pad23)")
  (net 26 "unconnected-(U1-Pad24)")
  (net 27 "unconnected-(U1-Pad25)")
  (net 28 "unconnected-(U1-Pad27)")
  (net 29 "unconnected-(U1-Pad28)")
  (net 30 "unconnected-(U1-Pad30)")
  (net 31 "unconnected-(U1-Pad29)")
  (net 32 "Net-(J2-Pad3)")
  (net 33 "Net-(R1-Pad2)")

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 0aa70a24-1d5b-43f2-99f3-b1714fc7f52a)
    (at 144.78 53.34 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/c41a6d44-f99d-4f53-b51c-3b7668c1e7af")
    (attr through_hole)
    (fp_text reference "R1" (at 7.366 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f5881c0-cd18-48ee-b734-9fc646780ef5)
    )
    (fp_text value "180K" (at 3.81 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5a0e8fb0-01f2-49ab-8dc9-86484b088050)
    )
    (fp_text user "${REFERENCE}" (at 7.366 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8c5fdfe4-7881-43aa-b104-783c04c26c7c)
    )
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 5f7c53ad-a221-4a7c-aa56-8fe23dde6e72))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp 78b56b61-ef8f-4805-b97c-5ab5c0b411cc))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp 80823b21-219d-43da-b6eb-be181e3e16d4))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 91826a79-9cb2-4edd-a5c8-fe91e96594c6))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp 9999883f-bca9-4fb8-9d59-1f4e86adf902))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp a67fffe0-e2da-47db-a79f-53669da8ef0d))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 2d762416-0fa5-45c8-b5b4-51e6a65b28c3))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 3b4f1163-b1f9-496c-8d52-80f2dac9dc15))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 4b4a40a9-e876-40cb-8917-5a45ec732d9d))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp f6cbf457-e8d0-490a-926c-3328ae081c9c))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 7b7dce25-0f02-428d-957d-697166d3b2b3))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp 832e5022-d413-40da-a7a8-e029faf6ea3b))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 9c78b812-39a8-4f2a-8b3d-34602766fbc7))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp a4b40906-1bd0-4936-99d1-42f01714592a))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp c068c0ae-9ea8-492e-af1d-bf4beb1f230c))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp df8af41a-a631-4bd2-9d38-31cd41f1aec4))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad1)") (pintype "passive") (tstamp 3f9ba76a-e880-4988-91ed-4af51b2b79d6))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R1-Pad2)") (pintype "passive") (tstamp 04843843-6452-4ee8-a167-6a9f24d0ee39))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Diode_THT:D_A-405_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5) (tstamp 461b57ca-6e57-4c93-acf1-d83265db0913)
    (at 144.78 93.98 -90)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/60960af7-b938-44a8-82b5-e9c36f2e6817")
    (attr through_hole)
    (fp_text reference "D1" (at 5.08 -2.47 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b95eb726-b792-43e1-99c3-bacc427fda9b)
    )
    (fp_text value "D" (at 5.08 2.47 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 333553c6-f6b4-4017-9145-356b55a50352)
    )
    (fp_text user "K" (at 0 -1.9 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e73019f4-013d-46d6-b03e-f5996a46ff27)
    )
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 096b0721-59af-4069-b366-cbe5ada38e92)
    )
    (fp_text user "K" (at 0 -1.9 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1254e6b1-b3d8-4078-82aa-bc62c7325b5d)
    )
    (fp_line (start 3.26 -1.47) (end 3.26 1.47) (layer "F.SilkS") (width 0.12) (tstamp 26cd95fd-c582-4d2b-af90-b4b9d8e785b1))
    (fp_line (start 7.8 1.47) (end 7.8 -1.47) (layer "F.SilkS") (width 0.12) (tstamp 2e090f0c-39de-4e7d-ba9f-b2774b7f9850))
    (fp_line (start 2.36 1.47) (end 7.8 1.47) (layer "F.SilkS") (width 0.12) (tstamp 3bbb2c92-e5f4-4bf4-b8dd-8a77829cbd1e))
    (fp_line (start 7.8 -1.47) (end 2.36 -1.47) (layer "F.SilkS") (width 0.12) (tstamp 3d8971b5-7b8d-4d63-993b-cc6f7ea3367a))
    (fp_line (start 1.14 0) (end 2.36 0) (layer "F.SilkS") (width 0.12) (tstamp 52f6a4eb-ea00-4024-ab99-c8d0cd1a5e9c))
    (fp_line (start 3.14 -1.47) (end 3.14 1.47) (layer "F.SilkS") (width 0.12) (tstamp 7ba4d48f-5451-440b-8a8e-22fe7eef120b))
    (fp_line (start 2.36 -1.47) (end 2.36 1.47) (layer "F.SilkS") (width 0.12) (tstamp 96432fed-9c8d-4296-aaa6-abceb311b7b2))
    (fp_line (start 3.38 -1.47) (end 3.38 1.47) (layer "F.SilkS") (width 0.12) (tstamp 9be50b51-d2d3-4959-acbd-a507e7a36dbc))
    (fp_line (start 9.02 0) (end 7.8 0) (layer "F.SilkS") (width 0.12) (tstamp ae635953-8a37-4026-b1d4-214eca6281c4))
    (fp_line (start -1.15 1.6) (end 11.31 1.6) (layer "F.CrtYd") (width 0.05) (tstamp 0055bec8-6166-4e38-8b42-7c8d052bbb28))
    (fp_line (start 11.31 1.6) (end 11.31 -1.6) (layer "F.CrtYd") (width 0.05) (tstamp 6e5ba312-84c6-4ee9-afaf-636ad43f0851))
    (fp_line (start 11.31 -1.6) (end -1.15 -1.6) (layer "F.CrtYd") (width 0.05) (tstamp 9be6514c-e6c3-4942-bca3-09fda2a89dbf))
    (fp_line (start -1.15 -1.6) (end -1.15 1.6) (layer "F.CrtYd") (width 0.05) (tstamp bba0662b-5ed9-49b7-84fb-6d3883e8411e))
    (fp_line (start 7.68 -1.35) (end 2.48 -1.35) (layer "F.Fab") (width 0.1) (tstamp 3b59f7f0-d674-48b6-bdfb-c2165b3d7fc5))
    (fp_line (start 10.16 0) (end 7.68 0) (layer "F.Fab") (width 0.1) (tstamp 54d41b06-3807-4c8b-8db1-7272dc1cbca8))
    (fp_line (start 3.16 -1.35) (end 3.16 1.35) (layer "F.Fab") (width 0.1) (tstamp 8139e267-9b2e-419e-9ccc-e348ee347764))
    (fp_line (start 3.26 -1.35) (end 3.26 1.35) (layer "F.Fab") (width 0.1) (tstamp 8e97bc1e-153e-4eab-b03e-81f844807a93))
    (fp_line (start 7.68 1.35) (end 7.68 -1.35) (layer "F.Fab") (width 0.1) (tstamp 9db0499f-ac6a-4bfc-a51c-40a61084e29f))
    (fp_line (start 0 0) (end 2.48 0) (layer "F.Fab") (width 0.1) (tstamp adb5f236-dda7-4106-af5b-32c5536b27c2))
    (fp_line (start 2.48 -1.35) (end 2.48 1.35) (layer "F.Fab") (width 0.1) (tstamp cee7a966-fd2b-4878-9304-49f4fa64ad08))
    (fp_line (start 3.36 -1.35) (end 3.36 1.35) (layer "F.Fab") (width 0.1) (tstamp d6c38841-3c40-43d5-a10f-0f65d2eb0bb3))
    (fp_line (start 2.48 1.35) (end 7.68 1.35) (layer "F.Fab") (width 0.1) (tstamp e86f4429-ccc1-486d-ae2a-3163f948e52a))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 05634166-2101-4e4a-995a-2e587833c72b))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 61748964-26e8-43dd-846d-345316e4275b))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Node_mcu:NodeMCU_SBC" (layer "F.Cu")
    (tedit 6235083C) (tstamp 7d77699c-7b66-4b9a-8778-d397edbf0c0b)
    (at 149.7375 58.42)
    (descr "NodeMCU ESP866")
    (tags "NodeMCU ESP866")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/bac5560b-af16-4666-9571-395f111e9db7")
    (attr through_hole)
    (fp_text reference "U1" (at 11.43 15.24) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f3275ef-5dfc-4708-a89a-d1593480bd29)
    )
    (fp_text value "NodeMCU_ESP32" (at 11.43 17.78) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3d003909-b06e-4543-9c7d-af64d1d376c2)
    )
    (fp_text user "D26" (at 2.54 20.32) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 03e6c7fb-acfb-40db-b061-4cc553e01c78)
    )
    (fp_text user "EN" (at 2.54 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 047828f7-e145-4486-ba1e-32aecdd05a0f)
    )
    (fp_text user "TX0" (at 22.86 5.08) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1412a3a4-4ab3-4e93-bc40-90cd19d7cf5d)
    )
    (fp_text user "D2" (at 22.86 27.94) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1d0529ce-bcb2-4156-88c8-ec166100bfd8)
    )
    (fp_text user "VIN" (at 2.54 35.56) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 24b6c2a2-8b57-49f7-8e2c-8703e8dd5bd0)
    )
    (fp_text user "TX2" (at 22.86 20.32) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 25f453d4-3ab6-400f-bb02-f3105c719532)
    )
    (fp_text user "D18" (at 22.86 15.24) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2bc44756-cc72-4dde-b999-b49d0cb38b5c)
    )
    (fp_text user "GND" (at 22.86 33.02) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 31a92b95-fc02-414b-8d09-d5c3b8181dce)
    )
    (fp_text user "D23" (at 22.86 0) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 32fc9cea-0ba4-45be-9621-5be6b7164914)
    )
    (fp_text user "D25" (at 2.54 17.78) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3452817a-ee5d-476f-a9b3-6d3f84a56f3a)
    )
    (fp_text user "D14" (at 2.54 25.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 391f407d-d263-4ada-93ec-1e5797f98bc7)
    )
    (fp_text user "3V3" (at 22.86 35.56) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 422de1f4-c1f7-404b-8462-711a2aa62094)
    )
    (fp_text user "D19" (at 22.86 12.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 44beb3c7-1318-4995-b3de-b6b00cede289)
    )
    (fp_text user "D34" (at 2.54 7.62) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 511cfb40-722e-4492-a39b-290ff96f1ce7)
    )
    (fp_text user "D35" (at 2.54 10.16) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 53db0102-aa02-45f1-aeb5-067d3a00cde4)
    )
    (fp_text user "D22" (at 22.86 2.54) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 587e93eb-6917-487b-a6f6-aa48e3a6dc4b)
    )
    (fp_text user "D21" (at 22.86 10.16) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 61eb2060-a830-4df8-8d19-b27bf9d534b1)
    )
    (fp_text user "RX2" (at 22.86 22.86) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 82b94bdd-2423-415a-8cf3-f9a4c27fddf3)
    )
    (fp_text user "D4" (at 22.86 25.4) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8ef2b0fc-dca0-44fc-846e-e622cf208603)
    )
    (fp_text user "D12" (at 2.54 27.94) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8f595a3d-ef11-4c36-bdf0-f8dad010c7a0)
    )
    (fp_text user "D33" (at 2.54 15.24) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 96d3c47e-9e8b-47f5-a7c9-bd33b79976d8)
    )
    (fp_text user "D32" (at 2.54 12.7) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a119d18d-10e3-49b1-bc68-181fad824cc6)
    )
    (fp_text user "D15" (at 22.86 30.48) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp acc3939f-acfa-4874-8a00-a5e7ca624456)
    )
    (fp_text user "D5" (at 22.86 17.78) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b44dddb5-6b9f-45d3-87b0-5a2fb50195e9)
    )
    (fp_text user "GND" (at 2.54 33.02) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d0434dcd-51c9-49e8-a7d5-ded091bd03c4)
    )
    (fp_text user "D13" (at 2.54 30.48) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d62cece6-5ce5-4c6a-b8bf-1028534d5283)
    )
    (fp_text user "VN" (at 2.54 5.08) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e43c73ff-a015-498d-8bd5-85b44b770fc5)
    )
    (fp_text user "D27" (at 2.54 22.86) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ec1a92c5-92d1-455f-8b83-e5fb01cc85ea)
    )
    (fp_text user "RX0" (at 22.86 7.62) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f0584821-e67b-40e4-ac3c-1f769baa5bd1)
    )
    (fp_text user "VP" (at 2.54 2.54) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fad205f3-6279-4373-8348-414292185556)
    )
    (fp_text user "${REFERENCE}" (at 11.43 15.24) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 17e221ca-ac6f-4b25-a4c4-7665deb8d327)
    )
    (fp_line (start 24.13 -1.27) (end 24.13 36.83) (layer "F.SilkS") (width 0.12) (tstamp 215e7771-8923-41a7-a5d1-f76a1e5930f2))
    (fp_line (start 1.27 36.83) (end 1.27 -1.27) (layer "F.SilkS") (width 0.12) (tstamp 3f074834-7552-4e85-acb3-38aa7e254b03))
    (fp_line (start 24.13 36.83) (end 26.67 36.83) (layer "F.SilkS") (width 0.12) (tstamp 76560d6a-cf21-47b7-bc05-5b361cd6b232))
    (fp_line (start -1.27 -1.27) (end -1.27 36.83) (layer "F.SilkS") (width 0.12) (tstamp 824e1be9-66f4-4cda-89b5-b0f51bbca45d))
    (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer "F.SilkS") (width 0.12) (tstamp 88bb05ce-a8bb-4128-affa-b74a7c2df80c))
    (fp_line (start 26.67 36.83) (end 26.67 -1.27) (layer "F.SilkS") (width 0.12) (tstamp 8fcb8644-bb85-42dd-8336-669926825aa8))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer "F.SilkS") (width 0.12) (tstamp a13bc25d-a83a-4ffb-93f2-391bdbf7478a))
    (fp_line (start -1.27 36.83) (end 1.27 36.83) (layer "F.SilkS") (width 0.12) (tstamp b46dccb1-f395-4251-ba92-5c4e90d06bff))
    (fp_line (start 26.67 -1.27) (end 24.13 -1.27) (layer "F.SilkS") (width 0.12) (tstamp bba2962c-78ca-423e-a31a-88b70d2c54b5))
    (fp_line (start -2.4875 -6.2) (end 27.8875 -6.2) (layer "F.CrtYd") (width 0.05) (tstamp 610fa838-b0a1-461d-8fa9-f3d17aeffb1f))
    (fp_line (start -2.4875 45.72) (end -2.4875 -6.2) (layer "F.CrtYd") (width 0.05) (tstamp a9f96fcd-2979-4501-9fcd-f691f774f001))
    (fp_line (start 27.8875 45.72) (end -2.4875 45.72) (layer "F.CrtYd") (width 0.05) (tstamp b0cab245-2338-4cf4-9b4f-8a92790d0cb7))
    (fp_line (start 27.8875 -6.2) (end 27.8875 45.72) (layer "F.CrtYd") (width 0.05) (tstamp b8a8d7a5-0179-4516-ae65-63e441904af7))
    (fp_line (start -1.8305 45.085) (end 27.2525 45.085) (layer "F.Fab") (width 0.1) (tstamp 0cc3c51a-1a70-4b5a-9249-7602211c71dc))
    (fp_line (start -0.762 -6.096) (end -1.778 -5.08) (layer "F.Fab") (width 0.1) (tstamp 9eead0e2-56ac-4c3d-844c-96ce64dac3a7))
    (fp_line (start 27.2525 45.085) (end 27.2525 -6.096) (layer "F.Fab") (width 0.1) (tstamp ad3e6a98-d1db-4bdd-bcf2-51abc7dcf9bb))
    (fp_line (start -1.8305 -5.08) (end -1.8305 45.085) (layer "F.Fab") (width 0.1) (tstamp eff6340a-d54b-45e7-a724-87f74b7322ca))
    (fp_line (start 27.2525 -6.096) (end -0.8145 -6.096) (layer "F.Fab") (width 0.1) (tstamp f15ef969-b708-4363-98e7-23a93def2e09))
    (pad "" np_thru_hole circle (at 25.3475 -4.25) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 0045065a-99e1-46d7-94ea-ec4be7c71d68))
    (pad "" np_thru_hole circle (at 25.3475 43.18) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp 6f98ff01-f5b3-4b25-9ed6-371f55ea098f))
    (pad "" np_thru_hole circle (at 0.1125 43.18) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp c115f35c-f98e-4600-a654-5d3d69844c99))
    (pad "" np_thru_hole circle (at 0.0625 -4.25) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask) (tstamp ca798cc9-36b7-4694-8792-454ae0768d1a))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "unconnected-(U1-Pad1)") (pinfunction "EN") (pintype "input+no_connect") (tstamp aa739f53-96c8-40a7-9101-8ff7d32a41b9))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad3)") (pinfunction "GPIO36/SENSOR_VP") (pintype "input") (tstamp 901f297b-40ea-4ae4-95f1-25a90c2a544e))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(R1-Pad2)") (pinfunction "GPIO39/SENSOR_VN") (pintype "input") (tstamp fae10d68-314a-406d-8b5b-4316304c51ae))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "unconnected-(U1-Pad4)") (pinfunction "GPIO34/VDET_1") (pintype "input+no_connect") (tstamp 7dbd067b-ca72-4941-b6ea-96e7fe65bd5f))
    (pad "5" thru_hole circle (at 0 10.16) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "unconnected-(U1-Pad5)") (pinfunction "GPIO35/VDET_2") (pintype "input+no_connect") (tstamp 3ce65260-8182-418a-a7b2-4f37060611ce))
    (pad "6" thru_hole circle (at 0 12.7) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "unconnected-(U1-Pad6)") (pinfunction "GPIO32") (pintype "bidirectional+no_connect") (tstamp 5f15fa2c-fe87-46d8-a652-e0d24bc4f661))
    (pad "7" thru_hole circle (at 0 15.24) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "unconnected-(U1-Pad7)") (pinfunction "GPIO33") (pintype "bidirectional+no_connect") (tstamp e49def2b-5f03-449a-8c59-a4747b02a841))
    (pad "8" thru_hole circle (at 0 17.78) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "unconnected-(U1-Pad8)") (pinfunction "GPIO25") (pintype "bidirectional+no_connect") (tstamp 5e0b2a0e-375a-45eb-ae50-9fe4936359df))
    (pad "9" thru_hole circle (at 0 20.32) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "unconnected-(U1-Pad9)") (pinfunction "GPIO26") (pintype "bidirectional+no_connect") (tstamp cb1a0346-16cf-4eae-aeba-50e4cf1d7d5a))
    (pad "10" thru_hole circle (at 0 22.86) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "unconnected-(U1-Pad10)") (pinfunction "GPIO27") (pintype "bidirectional+no_connect") (tstamp 5da11d55-848a-4c7c-8f5e-5413d2d2f8c3))
    (pad "11" thru_hole circle (at 0 25.4) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "unconnected-(U1-Pad11)") (pinfunction "GPIO14") (pintype "bidirectional+no_connect") (tstamp 03262628-1cc5-491d-862f-0eb1bd93094e))
    (pad "12" thru_hole circle (at 0 27.94) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U1-Pad12)") (pinfunction "GPIO12") (pintype "bidirectional+no_connect") (tstamp bd87c8ae-c0f8-478e-afa3-98b6cb999a88))
    (pad "13" thru_hole circle (at 0 30.48) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad2)") (pinfunction "GPIO13") (pintype "bidirectional") (tstamp dd9956f2-e1a3-43eb-b682-c9200e10a75b))
    (pad "14" thru_hole circle (at 0 33.02) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)") (pinfunction "GND") (pintype "power_in") (tstamp 2323f79f-5f15-4c4c-a037-a5f8decb05bf))
    (pad "15" thru_hole circle (at 0 35.56) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "Vin") (pintype "power_in") (tstamp 2c430825-f89e-46dd-92c0-a1eb7a4e3d36))
    (pad "16" thru_hole circle (at 25.4 35.56) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad16)") (pinfunction "3.3V") (pintype "power_out") (tstamp c567d4b7-eb8f-474d-bcf2-046b5758a4ae))
    (pad "17" thru_hole circle (at 25.4 33.02) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad17)") (pinfunction "GND") (pintype "power_in") (tstamp 8382be0b-64da-434d-b3bb-5bc1d436be2d))
    (pad "18" thru_hole circle (at 25.4 30.48) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad18)") (pinfunction "GPIO15") (pintype "bidirectional") (tstamp fbd23587-9e1b-4461-b511-2257604d25ff))
    (pad "19" thru_hole circle (at 25.4 27.94) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad19)") (pinfunction "GPIO2") (pintype "bidirectional") (tstamp 73012d62-09f7-4e13-998e-800cf36a3c2b))
    (pad "20" thru_hole circle (at 25.4 25.4) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "unconnected-(U1-Pad20)") (pinfunction "GPIO4") (pintype "bidirectional+no_connect") (tstamp 0dee7dc7-28b8-43a0-982f-9fa20c03186e))
    (pad "21" thru_hole circle (at 25.4 22.86) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-Pad21)") (pinfunction "RX2") (pintype "bidirectional+no_connect") (tstamp 790da2d6-8e50-4f89-a27a-5123b485dd01))
    (pad "22" thru_hole circle (at 25.4 20.32) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U1-Pad22)") (pinfunction "TX2") (pintype "bidirectional+no_connect") (tstamp 3051299b-281a-4da9-af5e-df120d6be2e6))
    (pad "23" thru_hole circle (at 25.4 17.78) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U1-Pad23)") (pinfunction "GPIO5") (pintype "bidirectional+no_connect") (tstamp f1cf15a4-7d3d-445f-8e3b-e019c22b3610))
    (pad "24" thru_hole circle (at 25.4 15.24) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U1-Pad24)") (pinfunction "GPIO18") (pintype "bidirectional+no_connect") (tstamp 843311f1-0d58-4820-882a-60bd65feb78f))
    (pad "25" thru_hole circle (at 25.4 12.7) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "unconnected-(U1-Pad25)") (pinfunction "GPIO19") (pintype "bidirectional+no_connect") (tstamp 51128b1c-82e7-4dff-a029-ff5ad1af097b))
    (pad "26" thru_hole circle (at 25.4 10.16) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U1-Pad26)") (pinfunction "GPIO21") (pintype "bidirectional+no_connect") (tstamp c0cda2c9-6149-436a-9d5d-b7ff307b5371))
    (pad "27" thru_hole circle (at 25.4 7.62) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "unconnected-(U1-Pad27)") (pinfunction "RX0") (pintype "bidirectional+no_connect") (tstamp 8da5761c-f46a-4b04-b82e-7fc6dac8f4c0))
    (pad "28" thru_hole circle (at 25.4 5.08) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "unconnected-(U1-Pad28)") (pinfunction "TX0") (pintype "bidirectional+no_connect") (tstamp fe9632fd-6344-4254-bb7c-69d57a7190da))
    (pad "29" thru_hole circle (at 25.4 2.54) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "unconnected-(U1-Pad29)") (pinfunction "GPIO22") (pintype "bidirectional+no_connect") (tstamp cd92f84f-b5ba-49f3-8483-c5aee648d32a))
    (pad "30" thru_hole circle (at 25.4 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "unconnected-(U1-Pad30)") (pinfunction "GPIO23") (pintype "bidirectional+no_connect") (tstamp d10264d7-2a3e-44dd-81a8-40c8b3dbe902))
    (model "${KISYS3DMOD}/Module.3dshapes/NodeMCU_Amica.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 96325eac-771c-4c16-ba14-694dd24fa9e5)
    (at 142.24 63.5 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/7e7b48e4-998f-4cd0-8159-bed4f4488c89")
    (attr through_hole)
    (fp_text reference "R2" (at 2.794 0 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c00665c7-238f-42f0-9cc8-e3a8fa63e130)
    )
    (fp_text value "12K" (at 6.35 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f1d6d2c-caeb-48e9-bf74-39571b5d016d)
    )
    (fp_text user "${REFERENCE}" (at 2.794 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6d29d228-5ab1-4850-93ed-cc89252531fb)
    )
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 1abff571-ce4a-491d-8731-be8e641e24c1))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 27fd3a94-0ef4-4671-8ce6-2763018dcefc))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp a308c690-ddb2-4f67-89b1-ae18f4a50d33))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp b7fc08a3-4bd7-4db0-a395-35de5dcdaa4a))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp e4a88fe3-b851-4450-91b8-576e32f280b2))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp f23d5b52-2046-4612-88da-619d8230a722))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 6e140721-4162-4217-9da4-cfa40a29762f))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 8870f5e5-b5fb-4e84-8f7f-f22a524bde42))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp b6ac3854-553b-4e0d-a4e5-e182f3d83e56))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp b9ace8ac-e175-4cf4-946c-1e81df63cb5f))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 242d8ecc-01f6-43ed-8ecf-5cdb857d8fd8))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp 2edd92c5-2c34-49cc-b521-df414cc7af89))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp 301db183-9684-486b-acdc-9e0c9ee1653d))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 3162c47d-3572-41f9-9aa1-1c7c65eb3adf))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 844c8ff1-4aea-44fc-8843-0a176c4dde02))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp c07e9c99-6d48-4e3a-a8e4-8bd21ad108ca))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R1-Pad2)") (pintype "passive") (tstamp a29d2e9b-9d04-4644-979e-7b300e66c13d))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)") (pintype "passive") (tstamp 656dcd69-9c0f-47a2-a2c4-765b804f50c1))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp ae8f59b6-c5dd-46dc-852a-e62d353873f6)
    (at 180.34 86.36)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/68d48ad4-88ad-4719-bd22-02147a9c50c3")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ca0abfa7-5775-47fb-9b2a-92bc21f12755)
    )
    (fp_text value "Conn_I2C" (at -2.54 10.16) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3b9386d1-0010-4e16-9053-3718b0a55307)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 526e5d6f-0df7-43c6-a5e5-aba48c38a164)
    )
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 0a4f01e7-4b70-400c-8c9d-1cdfb7f22bd8))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp 6b2de4c6-83fc-4a0b-8961-3132fb813080))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 8a9888d1-e4a7-4b64-a3e7-9d8e21085326))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp a7e9488f-f086-462a-9bb1-61029c365678))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp b3d9787f-99a9-4974-9405-bd3f1d9975ba))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp e8bd73e3-54bf-488d-8d2a-baf97328680b))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 0fa9bc68-b6d9-41cb-9e43-975a3c0b0ea5))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 4ea6d23e-7512-463e-8d54-e342b0ff89ad))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 90396c05-ad39-4619-86d0-537722b683fb))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp c04396e1-0c6c-4aa0-8f03-4fc619a2bc27))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 336cb3e1-c411-4000-a39d-7b674b45ccab))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 4b00516e-fa1b-4292-801f-b47786730295))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 5ea430ff-9dca-466e-82f6-83c246f88745))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 780760a6-f94a-49d9-9665-288cd1a04ac4))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp b8437e96-0da5-4663-8d24-5d248001bc2f))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad19)") (pinfunction "SDA") (pintype "bidirectional") (tstamp 544e7fb2-1f2d-487d-8a99-b570aac351d9))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad16)") (pinfunction "VCC") (pintype "power_in") (tstamp ee32e8cd-ab26-47ba-9b8d-45f12cfe08f7))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad18)") (pinfunction "SCL") (pintype "input") (tstamp 79172b03-8790-4156-9fff-e6572285b556))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad17)") (pinfunction "GND") (pintype "power_in") (tstamp 77f395a0-e150-4ffb-8ea1-5c603da24925))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp be3a8a3f-7fae-4c0b-934b-4361acb787a4)
    (at 144.78 50.8)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/013b7fe0-c393-480f-8f21-7b7e62b335e8")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 325bea33-ac9d-4c20-be3e-1d9cb21bae5f)
    )
    (fp_text value "Conn_battery" (at 0 2.33) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 514871b5-a5ae-4e63-9804-53d85f7ec10f)
    )
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f9070a1d-902a-41a3-a139-97b9cee9fea5)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 169e9081-26b8-4efc-8822-c2a98018aad9))
    (fp_line (start 1.33 1.27) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 1b9cdb86-19c4-433d-9e1d-5be4d5b70aab))
    (fp_line (start -1.33 1.27) (end -1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 6fdf8241-4bde-4264-be1e-127bbe0b8696))
    (fp_line (start -1.33 1.33) (end 1.33 1.33) (layer "F.SilkS") (width 0.12) (tstamp 9f6adb82-54ff-493d-a299-936e4f854946))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp d85ee29c-b5de-4863-81e9-0f52df99d2ab))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp e1d5acd0-4b34-453b-bc6c-7077862e0d4e))
    (fp_line (start -1.8 -1.8) (end -1.8 1.8) (layer "F.CrtYd") (width 0.05) (tstamp 2ac172c9-0d48-4bad-bba4-686054be36db))
    (fp_line (start -1.8 1.8) (end 1.8 1.8) (layer "F.CrtYd") (width 0.05) (tstamp 36e947d8-9a67-411b-a538-28849f4ee409))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 44590aa6-4756-43f6-b4d2-6c6ca642e8ef))
    (fp_line (start 1.8 1.8) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 88f5f093-7d51-4ba0-a86f-62166cbc97f3))
    (fp_line (start 1.27 -1.27) (end 1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 3acd1d09-7fc9-4a1f-a5a5-37e07d950b90))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 4b190fd6-2f6b-4a84-b1ce-7ae7ccd5285f))
    (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer "F.Fab") (width 0.1) (tstamp 9360c86a-c140-452e-9c85-f713fb43357e))
    (fp_line (start -1.27 1.27) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp ea8cfc8e-0a13-4a17-8b36-8638ace3b8e0))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp f3061990-d6ed-4907-a612-ef6acd556808))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad1)") (pinfunction "batt_36V") (pintype "power_out") (tstamp 2134e570-b5c4-4028-91d4-13cde2d1df9a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp bf2d82e4-234d-4669-9c08-250615d5ff59)
    (at 142.24 104.14 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/c6193a3d-ac57-49c6-9f84-c0f0df6baf32")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d7b271b2-bad3-4eb7-bdf1-cae86ca2a652)
    )
    (fp_text value "Conn_alim" (at -5.08 -2.54 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 58b22a9b-e7d9-4786-be37-9945fa44937e)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f7fcd9df-e987-44de-86f8-0b40acaf9c03)
    )
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 42b9aca4-d05f-416d-aafd-c8fb960c38a1))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 454aaa95-5766-48c8-a7b1-6553a0c51369))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 509196f5-f0cc-4a94-b44e-d0bd1b3ac676))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 6d2c1903-5d66-4fe4-874a-496cb530ec51))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp a16c5fd8-300b-40a5-88fb-a24658530f16))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp a4838db3-ef2f-4ff9-98b9-a5dcdcaa30e0))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 48f88f0a-d479-4b34-a517-302e22f787ca))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp cb92565d-81a4-40d4-960f-2e2b735c83c5))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp eee00f2a-f107-46a3-a62d-e9c4122ba67d))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp f0aa5d05-332d-4f13-944c-efbc829b3071))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 4cb9576d-cb2b-4b5b-a073-fdff4d716a86))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 7762a6b0-d285-4738-a679-afaa3f5ed1df))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ad770ff2-26e8-48a4-bdcd-7a1615b78423))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp bd5c2bd6-89e6-4e18-b8eb-e5cac8988ea6))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp d5706f8a-fee6-46a2-9a9e-2bcd9396c389))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "5V") (pintype "power_out") (tstamp 52f0d0f7-bcb6-4d9e-8560-9aede11ee9f8))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)") (pinfunction "GND") (pintype "power_out") (tstamp 097e8ab2-c652-48c5-ab67-0e505bed43e9))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp c6dbba4a-7e56-4cb4-9c10-0177346f251b)
    (at 165.1 48.26 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/5146355b-d187-42d7-bcfd-5946aeb905a6")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 808937ff-2c3b-4edc-a1b8-751965824410)
    )
    (fp_text value "Conn_speed_sensor" (at 2.54 4.87) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8f0ffab7-ddab-4d5d-9437-30e3f1806211)
    )
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0fc8dcc2-b6bb-480a-9765-fc686c30e69f)
    )
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 0fc63cee-d17e-49c5-b752-c80c3a365464))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp 1146882d-42c6-4e09-9ced-373d21c743eb))
    (fp_line (start -1.33 1.27) (end -1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 1994c1ea-57a8-4d05-8c31-42fca19c41e2))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 3e087e04-a8e2-4c0f-a8b4-cf005b628ee3))
    (fp_line (start 1.33 1.27) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp 579a4bac-69dc-433d-a731-e283bfdc356c))
    (fp_line (start -1.33 3.87) (end 1.33 3.87) (layer "F.SilkS") (width 0.12) (tstamp a29f9b85-fc86-449f-ade1-c75876b7ac95))
    (fp_line (start -1.8 4.35) (end 1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 4b00ecc2-6704-488c-9933-dfa8a6bed464))
    (fp_line (start -1.8 -1.8) (end -1.8 4.35) (layer "F.CrtYd") (width 0.05) (tstamp 70ce59f9-e01c-4644-9298-11231313de3c))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 773dd21e-1cd6-4f8d-b070-dc673e8422dc))
    (fp_line (start 1.8 4.35) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp b5490bbb-7f9f-4d69-890c-aa41188a8ee5))
    (fp_line (start 1.27 -1.27) (end 1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp 179d9469-e479-47f4-b192-26a506747917))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 6fd5e3a9-c40b-4c6d-9a06-6161d1e01711))
    (fp_line (start -1.27 3.81) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 717b1d74-42dc-43ed-a694-f8f0c4ba18b8))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp ac3491dc-0c1f-412f-af53-30d7305c31cd))
    (fp_line (start 1.27 3.81) (end -1.27 3.81) (layer "F.Fab") (width 0.1) (tstamp d000d5ae-8f47-4813-a5b9-bd578a111710))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)") (pinfunction "C1") (pintype "passive") (tstamp 636b7343-9253-405f-bcd8-80d60236acab))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad2)") (pinfunction "C2") (pintype "passive") (tstamp 6d1f2436-ed88-410c-9b41-e6c4f346a55c))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC) (tstamp decdcd19-79f8-476b-9690-33c944495a72)
    (at 160.02 48.26 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "MCU_board.kicad_sch")
    (property "Sheetname" "")
    (path "/9b0c1c36-20df-4c06-9ad3-2271ca2f63a2")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 022f95f1-5627-4183-8895-281467bf12a8)
    )
    (fp_text value "Conn_HSTS016L" (at -2.54 2.54 180) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp aefbab52-ffa8-43be-9197-a2369b46f6f8)
    )
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 34b35827-1fa7-49ed-a1a9-304569dfd4af)
    )
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 1d12f65e-74f2-4f76-93fb-1692907aa8a0))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer "F.SilkS") (width 0.12) (tstamp 7be066e5-e956-49e6-a8a4-ac4c102ed04a))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer "F.SilkS") (width 0.12) (tstamp d54b9676-a223-4987-9a06-03ef07d76a35))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp e78fa873-366f-47d5-83e7-715a6ad05ab7))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp f11cbf6c-5529-4b0b-a1f5-fcc301eb6185))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer "F.SilkS") (width 0.12) (tstamp f923f09d-a18f-4387-b851-d8c045ab7256))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp 15b1427e-5249-44eb-833c-0af53cd3b214))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp 8c8e3e96-c7fc-4108-9713-95fb137babb3))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer "F.CrtYd") (width 0.05) (tstamp f27b5181-3b76-4f0e-979c-bcabf1211e10))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer "F.CrtYd") (width 0.05) (tstamp f326c96d-f545-4622-b5aa-9c634527f4af))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp 0f654d55-2966-4eef-af22-38f84bc79f5e))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer "F.Fab") (width 0.1) (tstamp 29c76bb3-1a53-4297-8925-f484e6d94459))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer "F.Fab") (width 0.1) (tstamp 634eff02-e1c8-4143-aa90-120fca9b20c5))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer "F.Fab") (width 0.1) (tstamp c7195718-3193-459e-9197-14079c05f385))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp cda5f0c7-9067-46ca-865a-c2720b4d4083))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)") (pinfunction "GND") (pintype "power_in") (tstamp 3e78018f-453f-480d-871e-c0c3152a5885))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "5V") (pintype "power_in") (tstamp a07c521f-4806-4ad8-a904-4a8c01d0b3ed))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad3)") (pinfunction "Vout") (pintype "output") (tstamp cfad8a76-4b72-4446-9f7b-5f33cf40e087))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J2-Pad4)") (pinfunction "Vref") (pintype "output+no_connect") (tstamp 32ba3a41-7bc5-4813-b947-51b28f879fc1))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 139.7 43.18) (end 183 109.22) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp 01c517db-db70-46d2-9618-e9aeac9589c3))
  (dimension (type aligned) (layer "User.1") (tstamp a1df1579-7f98-456b-96b2-f2255e6a78f1)
    (pts (xy 139.7 109.22) (xy 139.7 43.18))
    (height -7.62)
    (gr_text "66.0400 mm" (at 130.93 76.2 90) (layer "User.1") (tstamp 8a962e46-a09b-4002-9560-1ec291e152f4)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1") (tstamp b74d18b6-0a0c-4ef4-b5e7-77a6be3fc614)
    (pts (xy 139.7 109.22) (xy 183 109.22))
    (height 5.08)
    (gr_text "43.3000 mm" (at 161.35 113.15) (layer "User.1") (tstamp 203eff38-5c86-45d7-8b0e-36659897a8dd)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 157.48 93.98) (end 157.48 48.26) (width 0.25) (layer "F.Cu") (net 1) (tstamp 01646aa5-b054-43f1-b5f8-0f1ab9601ac9))
  (segment (start 144.78 93.98) (end 149.7375 93.98) (width 0.25) (layer "F.Cu") (net 1) (tstamp 234befff-2efc-47ae-9199-dfa21f7042bc))
  (segment (start 149.7375 93.98) (end 157.48 93.98) (width 0.25) (layer "F.Cu") (net 1) (tstamp 9c57a1e3-692e-4a52-b303-face8ab5ff78))
  (segment (start 142.24 104.14) (end 144.78 104.14) (width 0.25) (layer "F.Cu") (net 2) (tstamp aedd3b50-30bf-42bc-a8e9-3298072ae91b))
  (segment (start 160.02 45.72) (end 160.02 48.26) (width 0.25) (layer "F.Cu") (net 3) (tstamp 3ed0041b-48be-427d-8cdf-667405c53983))
  (segment (start 142.24 91.44) (end 149.7375 91.44) (width 0.25) (layer "F.Cu") (net 3) (tstamp 69aa9a5f-ac33-4bff-a4fe-ea232936c76d))
  (segment (start 142.24 53.34) (end 142.24 45.72) (width 0.25) (layer "F.Cu") (net 3) (tstamp 9d0329ef-05c6-47e5-8ef7-8e218db685e3))
  (segment (start 142.24 45.72) (end 160.02 45.72) (width 0.25) (layer "F.Cu") (net 3) (tstamp a8a21ecc-ad8a-4cd7-bb90-f4a238c3160c))
  (segment (start 160.02 48.26) (end 165.1 48.26) (width 0.25) (layer "F.Cu") (net 3) (tstamp ab57be61-3be2-49a1-b1a4-004ab8e0694b))
  (segment (start 142.24 91.44) (end 142.24 68.58) (width 0.25) (layer "F.Cu") (net 3) (tstamp ac3b046c-2978-4d9a-839e-4f009b6edb92))
  (segment (start 142.24 101.6) (end 142.24 91.44) (width 0.25) (layer "F.Cu") (net 3) (tstamp f3c6f12c-d7a9-419e-944d-2f651ba46531))
  (segment (start 142.24 68.58) (end 143.51 67.31) (width 0.25) (layer "F.Cu") (net 3) (tstamp fe601422-18d3-4f37-bb00-5caa5362248b))
  (via (at 143.51 67.31) (size 0.8) (drill 0.4) (layers "F.Cu" "B.Cu") (net 3) (tstamp 32062560-499b-44dc-9b07-a0809ef2ea64))
  (segment (start 143.51 54.61) (end 142.24 53.34) (width 0.25) (layer "B.Cu") (net 3) (tstamp 8b014bea-020e-4c32-8a2e-afb44e577967))
  (segment (start 143.51 67.31) (end 143.51 54.61) (width 0.25) (layer "B.Cu") (net 3) (tstamp a9881c4d-1698-40b0-8ef8-bcb44452f73f))
  (segment (start 144.78 50.8) (end 144.78 53.34) (width 0.25) (layer "F.Cu") (net 5) (tstamp 5259d978-b387-4967-b81c-f641c98585a8))
  (segment (start 175.1375 86.36) (end 180.34 86.36) (width 0.25) (layer "F.Cu") (net 6) (tstamp 2f3e6f8a-067b-4be4-8100-0ee3ba1aa8d6))
  (segment (start 182.245 88.9) (end 180.34 88.9) (width 0.25) (layer "F.Cu") (net 7) (tstamp 2b024001-3319-44c4-9a71-6abcf8cd2df7))
  (segment (start 182.245 96.52) (end 182.245 88.9) (width 0.25) (layer "F.Cu") (net 7) (tstamp 656afe21-3714-4d3e-b229-e0beb358d8aa))
  (segment (start 175.26 96.52) (end 175.1375 96.3975) (width 0.25) (layer "F.Cu") (net 7) (tstamp 75b0b0ae-baaa-40e8-8fd5-a33a1047c815))
  (segment (start 175.26 96.52) (end 182.245 96.52) (width 0.25) (layer "F.Cu") (net 7) (tstamp 7fe237e8-1d0d-433a-9b24-5ea976762c57))
  (segment (start 175.1375 96.3975) (end 175.1375 93.98) (width 0.25) (layer "F.Cu") (net 7) (tstamp 8f0c6a81-1452-45ce-b4b3-75e50b620399))
  (segment (start 180.34 91.44) (end 177.8 88.9) (width 0.25) (layer "F.Cu") (net 8) (tstamp 30709b2e-b777-45ae-a45c-e8627bbcdf60))
  (segment (start 177.8 88.9) (end 175.1375 88.9) (width 0.25) (layer "F.Cu") (net 8) (tstamp d91ae5d5-90c9-4521-8710-e306638e1d50))
  (segment (start 160.02 88.9) (end 149.7375 88.9) (width 0.25) (layer "B.Cu") (net 9) (tstamp 527346bb-ea73-4a6b-90c5-e15d8df2e57f))
  (segment (start 167.64 81.28) (end 160.02 88.9) (width 0.25) (layer "B.Cu") (net 9) (tstamp 8fd52544-866c-407e-990a-b7ff97bb39d0))
  (segment (start 167.64 48.26) (end 167.64 81.28) (width 0.25) (layer "B.Cu") (net 9) (tstamp e39b0b7f-91f8-45ca-b50b-563bff3dc7f3))
  (segment (start 180.34 93.98) (end 177.8 91.44) (width 0.25) (layer "F.Cu") (net 10) (tstamp 1d2462aa-204d-4f12-8e50-109c8d4bcd0e))
  (segment (start 177.8 91.44) (end 175.1375 91.44) (width 0.25) (layer "F.Cu") (net 10) (tstamp e157eb32-72f8-4fc3-ac67-cd2ba1737fc5))
  (segment (start 154.94 60.96) (end 149.7375 60.96) (width 0.25) (layer "F.Cu") (net 32) (tstamp 61e763ec-1c1c-4f1e-a003-f55d7ad04f9f))
  (segment (start 154.94 48.26) (end 154.94 60.96) (width 0.25) (layer "F.Cu") (net 32) (tstamp e5c077a6-2e6e-4ddb-9cdd-7189d5453897))
  (segment (start 144.78 63.5) (end 149.7375 63.5) (width 0.25) (layer "F.Cu") (net 33) (tstamp 30bfa64d-761b-4732-997d-bd4590e66c7b))
  (segment (start 144.78 63.5) (end 142.24 63.5) (width 0.25) (layer "F.Cu") (net 33) (tstamp 637d2d4b-a4e1-430d-a2a4-ddc364bed10f))

)
