456286418549768
Connector_PinHeader_2.54mm
PinHeader_1x01_P2.54mm_Horizontal
Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x01 2.54mm single row
0
1
1
Connector_PinHeader_2.54mm
PinHeader_1x01_P2.54mm_Vertical
Through hole straight pin header, 1x01, 2.54mm pitch, single row
Through hole pin header THT 1x01 2.54mm single row
0
1
1
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Horizontal
Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x02 2.54mm single row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical
Through hole straight pin header, 1x02, 2.54mm pitch, single row
Through hole pin header THT 1x02 2.54mm single row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x02 2.54mm single row style2 pin1 right
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Horizontal
Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x03 2.54mm single row
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical
Through hole straight pin header, 1x03, 2.54mm pitch, single row
Through hole pin header THT 1x03 2.54mm single row
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x03 2.54mm single row style1 pin1 left
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x03 2.54mm single row style2 pin1 right
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Horizontal
Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x04 2.54mm single row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical
Through hole straight pin header, 1x04, 2.54mm pitch, single row
Through hole pin header THT 1x04 2.54mm single row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x04 2.54mm single row style2 pin1 right
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Horizontal
Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x05 2.54mm single row
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical
Through hole straight pin header, 1x05, 2.54mm pitch, single row
Through hole pin header THT 1x05 2.54mm single row
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x05 2.54mm single row style1 pin1 left
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x05 2.54mm single row style2 pin1 right
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Horizontal
Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x06 2.54mm single row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical
Through hole straight pin header, 1x06, 2.54mm pitch, single row
Through hole pin header THT 1x06 2.54mm single row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x06 2.54mm single row style1 pin1 left
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x06 2.54mm single row style2 pin1 right
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Horizontal
Through hole angled pin header, 1x07, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x07 2.54mm single row
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical
Through hole straight pin header, 1x07, 2.54mm pitch, single row
Through hole pin header THT 1x07 2.54mm single row
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x07, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x07 2.54mm single row style1 pin1 left
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x07, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x07 2.54mm single row style2 pin1 right
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Horizontal
Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x08 2.54mm single row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical
Through hole straight pin header, 1x08, 2.54mm pitch, single row
Through hole pin header THT 1x08 2.54mm single row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x08 2.54mm single row style1 pin1 left
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Horizontal
Through hole angled pin header, 1x09, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x09 2.54mm single row
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical
Through hole straight pin header, 1x09, 2.54mm pitch, single row
Through hole pin header THT 1x09 2.54mm single row
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x09, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x09 2.54mm single row style1 pin1 left
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x09, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x09 2.54mm single row style2 pin1 right
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Horizontal
Through hole angled pin header, 1x10, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x10 2.54mm single row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical
Through hole straight pin header, 1x10, 2.54mm pitch, single row
Through hole pin header THT 1x10 2.54mm single row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x10, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x10 2.54mm single row style1 pin1 left
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x10, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x10 2.54mm single row style2 pin1 right
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Horizontal
Through hole angled pin header, 1x11, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x11 2.54mm single row
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical
Through hole straight pin header, 1x11, 2.54mm pitch, single row
Through hole pin header THT 1x11 2.54mm single row
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x11, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x11 2.54mm single row style1 pin1 left
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x11, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x11 2.54mm single row style2 pin1 right
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Horizontal
Through hole angled pin header, 1x12, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x12 2.54mm single row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical
Through hole straight pin header, 1x12, 2.54mm pitch, single row
Through hole pin header THT 1x12 2.54mm single row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x12, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x12 2.54mm single row style1 pin1 left
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x12, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x12 2.54mm single row style2 pin1 right
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Horizontal
Through hole angled pin header, 1x13, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x13 2.54mm single row
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical
Through hole straight pin header, 1x13, 2.54mm pitch, single row
Through hole pin header THT 1x13 2.54mm single row
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x13, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x13 2.54mm single row style1 pin1 left
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x13, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x13 2.54mm single row style2 pin1 right
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Horizontal
Through hole angled pin header, 1x14, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x14 2.54mm single row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical
Through hole straight pin header, 1x14, 2.54mm pitch, single row
Through hole pin header THT 1x14 2.54mm single row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x14 2.54mm single row style1 pin1 left
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x14 2.54mm single row style2 pin1 right
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Horizontal
Through hole angled pin header, 1x15, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x15 2.54mm single row
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical
Through hole straight pin header, 1x15, 2.54mm pitch, single row
Through hole pin header THT 1x15 2.54mm single row
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x15, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x15 2.54mm single row style1 pin1 left
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x15, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x15 2.54mm single row style2 pin1 right
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Horizontal
Through hole angled pin header, 1x16, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x16 2.54mm single row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical
Through hole straight pin header, 1x16, 2.54mm pitch, single row
Through hole pin header THT 1x16 2.54mm single row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x16, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x16 2.54mm single row style1 pin1 left
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x16, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x16 2.54mm single row style2 pin1 right
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Horizontal
Through hole angled pin header, 1x17, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x17 2.54mm single row
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical
Through hole straight pin header, 1x17, 2.54mm pitch, single row
Through hole pin header THT 1x17 2.54mm single row
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x17, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x17 2.54mm single row style1 pin1 left
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x17, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x17 2.54mm single row style2 pin1 right
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Horizontal
Through hole angled pin header, 1x18, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x18 2.54mm single row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical
Through hole straight pin header, 1x18, 2.54mm pitch, single row
Through hole pin header THT 1x18 2.54mm single row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x18, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x18 2.54mm single row style1 pin1 left
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x18, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x18 2.54mm single row style2 pin1 right
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Horizontal
Through hole angled pin header, 1x19, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x19 2.54mm single row
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical
Through hole straight pin header, 1x19, 2.54mm pitch, single row
Through hole pin header THT 1x19 2.54mm single row
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x19, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x19 2.54mm single row style1 pin1 left
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x19, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x19 2.54mm single row style2 pin1 right
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Horizontal
Through hole angled pin header, 1x20, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x20 2.54mm single row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical
Through hole straight pin header, 1x20, 2.54mm pitch, single row
Through hole pin header THT 1x20 2.54mm single row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x20, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x20 2.54mm single row style1 pin1 left
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x20, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x20 2.54mm single row style2 pin1 right
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Horizontal
Through hole angled pin header, 1x21, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x21 2.54mm single row
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical
Through hole straight pin header, 1x21, 2.54mm pitch, single row
Through hole pin header THT 1x21 2.54mm single row
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x21, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x21 2.54mm single row style1 pin1 left
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x21, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x21 2.54mm single row style2 pin1 right
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Horizontal
Through hole angled pin header, 1x22, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x22 2.54mm single row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical
Through hole straight pin header, 1x22, 2.54mm pitch, single row
Through hole pin header THT 1x22 2.54mm single row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x22, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x22 2.54mm single row style1 pin1 left
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x22, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x22 2.54mm single row style2 pin1 right
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Horizontal
Through hole angled pin header, 1x23, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x23 2.54mm single row
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical
Through hole straight pin header, 1x23, 2.54mm pitch, single row
Through hole pin header THT 1x23 2.54mm single row
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x23, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x23 2.54mm single row style1 pin1 left
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x23, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x23 2.54mm single row style2 pin1 right
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Horizontal
Through hole angled pin header, 1x24, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x24 2.54mm single row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical
Through hole straight pin header, 1x24, 2.54mm pitch, single row
Through hole pin header THT 1x24 2.54mm single row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x24, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x24 2.54mm single row style1 pin1 left
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x24, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x24 2.54mm single row style2 pin1 right
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Horizontal
Through hole angled pin header, 1x25, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x25 2.54mm single row
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical
Through hole straight pin header, 1x25, 2.54mm pitch, single row
Through hole pin header THT 1x25 2.54mm single row
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x25, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x25 2.54mm single row style1 pin1 left
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x25, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x25 2.54mm single row style2 pin1 right
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Horizontal
Through hole angled pin header, 1x26, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x26 2.54mm single row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical
Through hole straight pin header, 1x26, 2.54mm pitch, single row
Through hole pin header THT 1x26 2.54mm single row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x26, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x26 2.54mm single row style1 pin1 left
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x26, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x26 2.54mm single row style2 pin1 right
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Horizontal
Through hole angled pin header, 1x27, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x27 2.54mm single row
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical
Through hole straight pin header, 1x27, 2.54mm pitch, single row
Through hole pin header THT 1x27 2.54mm single row
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x27, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x27 2.54mm single row style1 pin1 left
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x27, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x27 2.54mm single row style2 pin1 right
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Horizontal
Through hole angled pin header, 1x28, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x28 2.54mm single row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical
Through hole straight pin header, 1x28, 2.54mm pitch, single row
Through hole pin header THT 1x28 2.54mm single row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x28, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x28 2.54mm single row style1 pin1 left
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x28, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x28 2.54mm single row style2 pin1 right
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Horizontal
Through hole angled pin header, 1x29, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x29 2.54mm single row
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical
Through hole straight pin header, 1x29, 2.54mm pitch, single row
Through hole pin header THT 1x29 2.54mm single row
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x29, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x29 2.54mm single row style1 pin1 left
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x29, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x29 2.54mm single row style2 pin1 right
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Horizontal
Through hole angled pin header, 1x30, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x30 2.54mm single row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical
Through hole straight pin header, 1x30, 2.54mm pitch, single row
Through hole pin header THT 1x30 2.54mm single row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x30, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x30 2.54mm single row style1 pin1 left
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x30, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x30 2.54mm single row style2 pin1 right
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Horizontal
Through hole angled pin header, 1x31, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x31 2.54mm single row
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical
Through hole straight pin header, 1x31, 2.54mm pitch, single row
Through hole pin header THT 1x31 2.54mm single row
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x31, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x31 2.54mm single row style1 pin1 left
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x31, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x31 2.54mm single row style2 pin1 right
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Horizontal
Through hole angled pin header, 1x32, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x32 2.54mm single row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical
Through hole straight pin header, 1x32, 2.54mm pitch, single row
Through hole pin header THT 1x32 2.54mm single row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x32, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x32 2.54mm single row style1 pin1 left
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x32, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x32 2.54mm single row style2 pin1 right
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Horizontal
Through hole angled pin header, 1x33, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x33 2.54mm single row
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical
Through hole straight pin header, 1x33, 2.54mm pitch, single row
Through hole pin header THT 1x33 2.54mm single row
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x33, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x33 2.54mm single row style1 pin1 left
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x33, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x33 2.54mm single row style2 pin1 right
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Horizontal
Through hole angled pin header, 1x34, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x34 2.54mm single row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical
Through hole straight pin header, 1x34, 2.54mm pitch, single row
Through hole pin header THT 1x34 2.54mm single row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x34, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x34 2.54mm single row style1 pin1 left
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x34, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x34 2.54mm single row style2 pin1 right
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Horizontal
Through hole angled pin header, 1x35, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x35 2.54mm single row
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical
Through hole straight pin header, 1x35, 2.54mm pitch, single row
Through hole pin header THT 1x35 2.54mm single row
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x35, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x35 2.54mm single row style1 pin1 left
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x35, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x35 2.54mm single row style2 pin1 right
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Horizontal
Through hole angled pin header, 1x36, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x36 2.54mm single row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical
Through hole straight pin header, 1x36, 2.54mm pitch, single row
Through hole pin header THT 1x36 2.54mm single row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x36, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x36 2.54mm single row style1 pin1 left
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x36, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x36 2.54mm single row style2 pin1 right
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Horizontal
Through hole angled pin header, 1x37, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x37 2.54mm single row
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical
Through hole straight pin header, 1x37, 2.54mm pitch, single row
Through hole pin header THT 1x37 2.54mm single row
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x37, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x37 2.54mm single row style1 pin1 left
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x37, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x37 2.54mm single row style2 pin1 right
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Horizontal
Through hole angled pin header, 1x38, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x38 2.54mm single row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical
Through hole straight pin header, 1x38, 2.54mm pitch, single row
Through hole pin header THT 1x38 2.54mm single row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x38, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x38 2.54mm single row style1 pin1 left
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x38, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x38 2.54mm single row style2 pin1 right
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Horizontal
Through hole angled pin header, 1x39, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x39 2.54mm single row
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical
Through hole straight pin header, 1x39, 2.54mm pitch, single row
Through hole pin header THT 1x39 2.54mm single row
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x39, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x39 2.54mm single row style1 pin1 left
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x39, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x39 2.54mm single row style2 pin1 right
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Horizontal
Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x40 2.54mm single row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical
Through hole straight pin header, 1x40, 2.54mm pitch, single row
Through hole pin header THT 1x40 2.54mm single row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x40, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x40 2.54mm single row style1 pin1 left
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x40, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x40 2.54mm single row style2 pin1 right
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Horizontal
Through hole angled pin header, 2x01, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Vertical
Through hole straight pin header, 2x01, 2.54mm pitch, double rows
Through hole pin header THT 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x01, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Horizontal
Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Vertical
Through hole straight pin header, 2x02, 2.54mm pitch, double rows
Through hole pin header THT 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Horizontal
Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Vertical
Through hole straight pin header, 2x03, 2.54mm pitch, double rows
Through hole pin header THT 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Horizontal
Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Vertical
Through hole straight pin header, 2x04, 2.54mm pitch, double rows
Through hole pin header THT 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Horizontal
Through hole angled pin header, 2x05, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Vertical
Through hole straight pin header, 2x05, 2.54mm pitch, double rows
Through hole pin header THT 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x05, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Horizontal
Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Vertical
Through hole straight pin header, 2x06, 2.54mm pitch, double rows
Through hole pin header THT 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x06, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Horizontal
Through hole angled pin header, 2x07, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Vertical
Through hole straight pin header, 2x07, 2.54mm pitch, double rows
Through hole pin header THT 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Horizontal
Through hole angled pin header, 2x08, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Vertical
Through hole straight pin header, 2x08, 2.54mm pitch, double rows
Through hole pin header THT 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x08, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Horizontal
Through hole angled pin header, 2x09, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Vertical
Through hole straight pin header, 2x09, 2.54mm pitch, double rows
Through hole pin header THT 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x09, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Horizontal
Through hole angled pin header, 2x10, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Vertical
Through hole straight pin header, 2x10, 2.54mm pitch, double rows
Through hole pin header THT 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x10, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Horizontal
Through hole angled pin header, 2x11, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Vertical
Through hole straight pin header, 2x11, 2.54mm pitch, double rows
Through hole pin header THT 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x11, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Horizontal
Through hole angled pin header, 2x12, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Vertical
Through hole straight pin header, 2x12, 2.54mm pitch, double rows
Through hole pin header THT 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x12, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Horizontal
Through hole angled pin header, 2x13, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Vertical
Through hole straight pin header, 2x13, 2.54mm pitch, double rows
Through hole pin header THT 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x13, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Horizontal
Through hole angled pin header, 2x14, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Vertical
Through hole straight pin header, 2x14, 2.54mm pitch, double rows
Through hole pin header THT 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x14, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Horizontal
Through hole angled pin header, 2x15, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Vertical
Through hole straight pin header, 2x15, 2.54mm pitch, double rows
Through hole pin header THT 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x15, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Horizontal
Through hole angled pin header, 2x16, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Vertical
Through hole straight pin header, 2x16, 2.54mm pitch, double rows
Through hole pin header THT 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x16, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Horizontal
Through hole angled pin header, 2x17, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Vertical
Through hole straight pin header, 2x17, 2.54mm pitch, double rows
Through hole pin header THT 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x17, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Horizontal
Through hole angled pin header, 2x18, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Vertical
Through hole straight pin header, 2x18, 2.54mm pitch, double rows
Through hole pin header THT 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x18, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Horizontal
Through hole angled pin header, 2x19, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Vertical
Through hole straight pin header, 2x19, 2.54mm pitch, double rows
Through hole pin header THT 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x19, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Horizontal
Through hole angled pin header, 2x20, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Vertical
Through hole straight pin header, 2x20, 2.54mm pitch, double rows
Through hole pin header THT 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x20, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Horizontal
Through hole angled pin header, 2x21, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Vertical
Through hole straight pin header, 2x21, 2.54mm pitch, double rows
Through hole pin header THT 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x21, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Horizontal
Through hole angled pin header, 2x22, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Vertical
Through hole straight pin header, 2x22, 2.54mm pitch, double rows
Through hole pin header THT 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x22, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Horizontal
Through hole angled pin header, 2x23, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Vertical
Through hole straight pin header, 2x23, 2.54mm pitch, double rows
Through hole pin header THT 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x23, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Horizontal
Through hole angled pin header, 2x24, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Vertical
Through hole straight pin header, 2x24, 2.54mm pitch, double rows
Through hole pin header THT 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x24, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Horizontal
Through hole angled pin header, 2x25, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Vertical
Through hole straight pin header, 2x25, 2.54mm pitch, double rows
Through hole pin header THT 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x25, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Horizontal
Through hole angled pin header, 2x26, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Vertical
Through hole straight pin header, 2x26, 2.54mm pitch, double rows
Through hole pin header THT 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x26, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Horizontal
Through hole angled pin header, 2x27, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Vertical
Through hole straight pin header, 2x27, 2.54mm pitch, double rows
Through hole pin header THT 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x27, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Horizontal
Through hole angled pin header, 2x28, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Vertical
Through hole straight pin header, 2x28, 2.54mm pitch, double rows
Through hole pin header THT 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x28, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Horizontal
Through hole angled pin header, 2x29, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Vertical
Through hole straight pin header, 2x29, 2.54mm pitch, double rows
Through hole pin header THT 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x29, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Horizontal
Through hole angled pin header, 2x30, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Vertical
Through hole straight pin header, 2x30, 2.54mm pitch, double rows
Through hole pin header THT 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x30, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Horizontal
Through hole angled pin header, 2x31, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Vertical
Through hole straight pin header, 2x31, 2.54mm pitch, double rows
Through hole pin header THT 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x31, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Horizontal
Through hole angled pin header, 2x32, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Vertical
Through hole straight pin header, 2x32, 2.54mm pitch, double rows
Through hole pin header THT 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x32, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Horizontal
Through hole angled pin header, 2x33, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Vertical
Through hole straight pin header, 2x33, 2.54mm pitch, double rows
Through hole pin header THT 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x33, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Horizontal
Through hole angled pin header, 2x34, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Vertical
Through hole straight pin header, 2x34, 2.54mm pitch, double rows
Through hole pin header THT 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x34, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Horizontal
Through hole angled pin header, 2x35, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Vertical
Through hole straight pin header, 2x35, 2.54mm pitch, double rows
Through hole pin header THT 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x35, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Horizontal
Through hole angled pin header, 2x36, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Vertical
Through hole straight pin header, 2x36, 2.54mm pitch, double rows
Through hole pin header THT 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x36, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Horizontal
Through hole angled pin header, 2x37, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Vertical
Through hole straight pin header, 2x37, 2.54mm pitch, double rows
Through hole pin header THT 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x37, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Horizontal
Through hole angled pin header, 2x38, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Vertical
Through hole straight pin header, 2x38, 2.54mm pitch, double rows
Through hole pin header THT 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x38, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Horizontal
Through hole angled pin header, 2x39, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Vertical
Through hole straight pin header, 2x39, 2.54mm pitch, double rows
Through hole pin header THT 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x39, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Horizontal
Through hole angled pin header, 2x40, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x40 2.54mm double row
0
80
80
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Vertical
Through hole straight pin header, 2x40, 2.54mm pitch, double rows
Through hole pin header THT 2x40 2.54mm double row
0
80
80
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x40, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x40 2.54mm double row
0
80
80
