(module NodeMCU_Amica (layer F.Cu) (tedit 5C2D2650)
  (descr "NodeMCU ESP866")
  (tags "NodeMCU ESP866")
  (fp_text reference REF** (at 11.43 15.24) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value NodeMCU_Amica (at 11.43 17.78) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VIN (at 2.54 35.56) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user G (at 2.54 33.02) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user RST (at 2.54 30.48) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user EN (at 2.54 27.94) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 3V (at 2.54 25.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user G (at 2.54 22.86) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SK (at 2.54 20.32) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SO (at 2.54 17.78) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user SC (at 2.54 15.24) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user S1 (at 2.54 12.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user S2 (at 2.54 10.16) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user S3 (at 2.54 7.62) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user VU (at 2.54 5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user G (at 2.54 2.54) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user A0 (at 2.54 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 3V (at 20.32 35.56) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user G (at 20.32 33.02) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user TX (at 20.32 30.48) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user RX (at 20.32 27.94) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D8 (at 20.32 25.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D7 (at 20.32 22.86) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D6 (at 20.32 20.32) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D5 (at 20.32 17.78) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user G (at 20.32 15.24) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 3V (at 20.32 12.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D4 (at 20.32 10.16) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D3 (at 20.32 7.62) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D2 (at 20.32 5.08) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D1 (at 20.32 2.54) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user D0 (at 20.32 0) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.8 42.4) (end -1.8 -6.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 24.6 42.4) (end -1.8 42.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 24.6 -6.2) (end 24.6 42.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 -6.2) (end 24.6 -6.2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.27 -1.27) (end -1.27 36.83) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.27 36.83) (end 1.27 36.83) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.27 36.83) (end 1.27 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.27 1.27) (end -1.27 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 21.59 36.83) (end 24.13 36.83) (layer F.SilkS) (width 0.12))
  (fp_line (start 21.59 -1.27) (end 21.59 36.83) (layer F.SilkS) (width 0.12))
  (fp_line (start 24.13 -1.27) (end 21.59 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 24.13 36.83) (end 24.13 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.143 -5.08) (end -1.143 42.164) (layer F.Fab) (width 0.1))
  (fp_line (start -1.143 42.164) (end 24.003 42.164) (layer F.Fab) (width 0.1))
  (fp_line (start 24.003 42.164) (end 24.003 -6.096) (layer F.Fab) (width 0.1))
  (fp_line (start 24.003 -6.096) (end -0.127 -6.096) (layer F.Fab) (width 0.1))
  (fp_text user %R (at 11.43 15.24) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -0.127 -6.096) (end -1.143 -5.08) (layer F.Fab) (width 0.1))
  (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 0 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0 20.32) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 0 22.86) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 25.4) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 0 27.94) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 0 30.48) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 33.02) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 0 35.56) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 22.86 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 22.86 30.48) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 22.86 33.02) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 22.86 27.94) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 22.86 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 22.86 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 22.86 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 22.86 35.56) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 22.86 20.32) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 22.86 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 22.86 22.86) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 22.86 25.4) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 22.86 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 22.86 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 22.86 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0.8 39.38) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 22 39.38) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 22 -4.25) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0.75 -4.25) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Module.3dshapes/NodeMCU_Amica.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
